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Fire prevention starts with recognizing hazards, controlling ignition sources, and knowing how to respond if a fire occurs.
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Introduction 
Open with: “Today’s safety topic is basic fire safety—because preventing a fire is safer than having to fight one.” Everyone has a role in controlling ignition sources and combustible materials.
Key Points: Prevent fires before they start. Know where fire extinguishers are located and how they are used.
Why It Matters 
Common workplace fire hazards include electrical problems, hot work, open flames, smoking, and improperly stored combustible or flammable materials.
Damaged cords and overloaded circuits can create ignition hazards.
Hot work or open flames can ignite nearby combustible materials.
	Quick Engagement Question: “Where is the nearest fire extinguisher, and what fire hazards are present in our work area today?”


Recognizing Fire Hazards 
Keep the discussion practical and focused on hazards employees can identify and correct before work begins.
	Common Fire Hazards
Damaged cords or overloaded circuits
Combustibles or flammables near hot work or heaters
Open flames, smoking, or improperly discarded matches/cigarettes
	Prevention Actions
Obey “No Smoking” signs and use proper receptacles
Remove damaged cords from service
Store flammables safely and clear combustibles before hot work
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	Mini Scenario: “You notice a damaged electrical cord beside combustible waste. What should you do before work continues?”


Fire Extinguishers & Response 
Use the correct extinguisher, know its location, and remember the P.A.S.S. method.
	P.A.S.S. Method
Pull the pin
Aim at the base
Squeeze the handle
Sweep side to side
	Inspection & Readiness
Maintenance tag current within 12 months
Visual inspection every 30 days
Replace discharged units and missing/damaged pins or seals
	What NOT to Do
Do not horseplay with extinguishers
Do not block extinguishers or leave combustibles in hot-work areas
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Fire Safety Reminders 
Know where fire-fighting equipment is located and keep required extinguishers accessible.
Keep extinguishers conspicuously placed and accessible.
Keep an extinguisher immediately available during hot work.
· Keep equipment properly lubricated to prevent excessive friction.
	Closing Message: “Basic fire safety is about prevention first. Control ignition sources, keep combustibles away from heat and hot work, and always know where the nearest fire extinguisher is located.”
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